HeHe Hansen - Rover - RPI
=========================

raspberry pi 3
camera module
gprs/gps module

## systeme
install Arch Linux ARM systeme on rpi following these how to : https://archlinuxarm.org/platforms/armv8/broadcom/raspberry-pi-3

connect to rpi through ssh

add alarm user to sudoers : https://wiki.archlinux.org/index.php/Sudo#Example_Entries
as root : ```pacman -S sudo``` then add "alarm ALL=(ALL) ALL" with visudo command

install git : ```pacman -S git```   
clone this repos : ```git clone -o guime https://g-u-i.me/gogs/bachir/hehe-rover.git ```

run rpi/install.sh with sudo

### what install is doing

- generate the locale : https://wiki.archlinux.org/index.php/Locale#Generating_locales
- make updates : ```pacman -Syyu```
- install vim rsync : ```pacman -S vim rsync```
- to be continued

## camera module
https://wiki.archlinux.org/index.php/Raspberry_Pi#Raspberry_Pi_camera_module


## gps
#### connection
https://github.com/embeddedartists/gps_shield   


#### package installation
i2c : https://wiki.archlinux.org/index.php/Raspberry_Pi#I2C
do not install ic2-tools from pacman, instead compile ic2-tools-git from aur as python-smbus depends on it.

```
cd ~
mkdir pkgs
cd pkgs

# i2c-tools
git clone https://aur.archlinux.org/i2c-tools-git.git
cd i2c-tools-git
makepkg -sri
cd ../

# python
pacman -S python

# python-smbus
git clone https://aur.archlinux.org/python-smbus.git
cd python-smbus
makepkg -sri

#pip
pacman -S python-pip

#nmea
pip install pynmea2

```


## gsm
